Brand: O/M 
Luminaire name: AS
Model: AS Recessed
Code: 15901
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005, .12 Brushed stainless steel

Design: Álvaro Siza
Emergency recessed luminaire with body made of stainless steel with brushed finish or electrostatic 100% polyester paint with textured-finish.
Pictogram, with acrylic structure and adhesive film, supplied separately.
The same luminaire allows maintained or non-maintained mode.
Luminaire with self-testing mode.
Prepared for remote control (rest mode).
3-hour autonomy.
Compliant with the following standards:
EN60598-2-22 / EN60598-1 / UNE 20392 

2,4W / 65lm / 5000K / Product /  / 375x120x100mm

Power supply included.
IP22 | 230Vac | 50/60Hz

LOR 19%, UGR , insulation class II