Brand: O/M 
Luminaire name: OS
Model: OS Wall-mounted
Code: 15909
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005

Design: Eduardo Souto de Moura
Emergency wall-mounted luminaire with body made of steel and electrostatic 100% polyester paint with textured finish.
Single sided pictogram, with polycarbonate structure and adhesive film, included.
The same luminaire allows maintained or non-maintained mode.
Luminaire with self-testing mode.
Prepared for remote control (rest mode).
3-hours autonomy.
Compliant with the following standards:
EN60598-2-22 / EN60598-1

2,4W / 65lm / 5000K / DALI /  / 346x98x123mm

Power supply included.
IP44 | IK07 | 230Vac | 50/60Hz

LOR 19%, UGR -, insulation class II