Brand: O/M 
Luminaire name: Beam
Model: Beam IP54
Code: 60401
Finishes: .04 Matt White, .05 Matt Black

Design: O/M
Ceiling-recessed luminaire made of aluminium die-cast.
Recessing accessory for flush version supplied separately.

10W / 670lm /  2700K / DALI / Medium 23° / ø75mm

LED CRI>90 / >50.000h, L80/B10
2-step MacAdam / power supply included
IP54 | 230Vac | 50/60Hz

LOR 70%, UGR <19, insulation class II