Brand: O/M 
Luminaire name: Dot
Model: Dot
Code: 60481
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005, .12 Brushed stainless steel, .34 Rust

Design: O/M
Ceiling-recessed luminaire, with aluminium body with 25micron maximum corrosion resistance anodization. Trim aluminium with matt finish or with textured electrostatic 100% polyester paint.
Tempered clear glass.
Supplied with cable (2x0,50mm²).
Driver to be ordered separately.

Values for 700mA. For 350mA estimate half of the indicated values.

2,2W / 145lm /  4000K / On/Off / Diffuse  / Ø36mm

LED CRI>80 / >50.000h, L80/B10 / 3-step MacAdam
IP67 | 350mA / 700mA

LOR 48%, UGR <28, insulation class III