Brand: O/M 
Luminaire name: Tubo Evo
Model: Tubo Evo
Code: 62501
Finishes: .20 Clear

Design: O/M
Surface luminaire with tubular shock-resistant clear polycarbonate diffuser and anti-condensation system comprising a valve that prevents condensation within the luminaire without affecting its high level of protection.
End caps in clear polycarbonate with marked installation angles.
Optic system with acrylic lens.
Equipped with 1m cable (H05RN-F) and a metallic cable gland.
Fitting accessories and IP68 connector supplied separately.

39W / 4100lm / 4000K / DALI / Flood 46° / 1037mm

LED CRI>80 />50.000h, L80/B10 / 3-step MacAdam
Power supply included.
IP67 | IK08| 230Vac | 50/60Hz

LOR 75%, UGR <13, insulation class I