Brand: O/M 
Luminaire name: 
Model: U60 IP54 Ceiling-mounted
Code: 34609
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005, .10 Anodised aluminium, .00 RAL on request

U60 IP54 Ceiling-mounted, LED / 29,5W / 4400lm / 3000K / 1150mm 



LOR= 48%, UGR <25, insulation class I. 
LED CRI>80 / >50.000h, L80/B10 / 3-step MacAdam
Power supply included.
IP54 | 230Vac | 50/60Hz
DALI
