Brand: O/M 
Luminaire name: Nub
Model: Nub
Code: 60001
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005

Design: O/M + Bartenbach GmbH
Ceiling-recessed luminaire with aluminium die-cast body with electrostatic 100% polyester paint finish. Focal lens with complex surfaces to provide a focal point through an 8mm aperture for low glare illumination. 
Driver to be ordered separately.

5,6W / 310lm / 2700K / On/Off / Flood 55° / ø28mm

LED CRI>90 / >50.000h, L80/B10
2-step MacAdam
IP65

LOR 67%, UGR <22, insulation class III