Brand: O/M 
Luminaire name: Nub
Model: Nub Flush 
Code: 60017
Finishes: .02 Black / RAL 9005

Design: O/M + Bartenbach GmbH
Ceiling-recessed luminaire with aluminium die-cast body with electrostatic 100% polyester paint finish.
Focal-lens with complex surfaces to provide a focal point through an 8mm aperture for low glare illumination.
Supplied with fermacell® plasterboard fiber recessing accessory or plasterboard.
Driver to be ordered separately.

5,6W / 290lm / 4000K / On/Off / Flood 58° / 8mm

LED CRI>90 / >50.000h, L80/B10
2-step MacAdam
IP65

LOR 59%, UGR <28, insulation class III