Brand: O/M 
Luminaire name: Over
Model: Over Track
Code: 60268
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005

Design: O/M + Bartenbach GmbH
Track-mounted spotlight with die-cast aluminium body with electrostatic 100% polyester paint finish.
Spot-lens with individual complex surface rips to provide a focal light and an extremely narrow beam.
Orientable by 90° horizontal rotation and 330° vertical rotation.
Driver included.

4,5W / 350lm /  2700K / On/Off / Medium 41° / ø85mm

LED CRI>90 / >50.000h, L80/B10
2-step MacAdam / Driver included.
IP20 | 230Vac | 50/60Hz

LOR 73%, UGR 230Vac, insulation class I