Brand: O/M 
Luminaire name: inVision35
Model: inVision35 Surface/Pendant
Code: 60654
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005

Design: O/M + Bartenbach GmbH
Surface or pendant luminaire with housing made of aluminium with electrostatic 100% polyester paint with textured finish.
Aluminium anodised end caps with matt finish or electrostatic 100% polyester paint with textured-finish.
Housing and perforated cover plate made of aluminium with textured-paint finish. With the latest Bartenbach GmbH technology, inVision35 is a discreet solution, that can use great light distribution and visual comfort from a nearly invisible source.
Fitting accessories for pendant version ordered separately.

27W / 1760lm / 2700K / On/Off / Medium 31° / 1211mm

LED CRI>90 / >50.000h, L80/B10 / 2-step MacAdam
Power supply included.
IP20 | 230Vac | 50/60Hz

LOR 73%, UGR <10, insulation class I