Brand: O/M 
Luminaire name: Tubo
Model: Tubo 50
Code: 62740
Finishes: .25 Frost

Design: Eduardo Souto de Moura
Surface or pendant luminaire with tubular shock-resistant frosted polycarbonate body with 50mm diameter.
Clear polycarbonate end caps with marked installation angles. Supplied with 30mm plastic cable gland that 
prevents condensation within luminaire.
Fitting accessories ordered separately.

24W / 3210lm / 3000K / On/Off / Diffuse / 1752mm

LED CRI>80 / >50.000h, L80/B10 / 3-step MacAdam
Power supply included.
IP67 | IK08 | 230Vac | 50/60Hz

LOR 75%, UGR <25, insulation class I