Brand: O/M 
Luminaire name: One
Model: One Trimless
Code: 63533
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005

Design: O/M + Bartenbach GmbH
Ceiling-recessed luminaire with aluminium die-cast body and heat sink with electrostatic 100% polyester paint finish.
Lightcore optics for defined and perfectly controlled beam of light.
Recessing accessory supplied separately.

3,1W / 230lm / 3000K / DALI / Flood 56° / ø39mm

LED CRI>90 / >50.000h, L80/B10
2-step MacAdam / Power supply included.
IP20 | 230Vac | 50/60Hz

LOR 88%, UGR <16, insulation class II