Brand: O/M 
Luminaire name: One
Model: One Adjustable
Code: 63563
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005

Design: O/M + Bartenbach GmbH
Ceiling-recessed luminaire with aluminium die-cast body and heat sink with electrostatic 100% polyester paint finish.
Orientable by 20° horizontal rotation.
Accurate reflector for a defined and controlled beam of light, achieving maximum efficiency. 

5,6W / 410lm / 2700K / On/Off / Medium 40° / ø60mm

LED CRI>90 / >50.000h, L80/B10
2-step MacAdam / Power supply included.
IP20 | 230Vac | 50/60Hz

LOR 89%, UGR <19, insulation class II