Brand: O/M 
Luminaire name: inFinit
Model: inFinit Pendant direct/indirect
Code: 63765
Finishes: .04 Matt White, .05 Matt Black

Design: OM + Bartenbach GmbH
Pendant direct and indirect luminaire with housing made of aluminium in matte finish.
Aluminium anodised end caps with matt finish. 
Linear extruded lenses (Lightstream) combined with a secondary reflector, integrated into an extruded aluminium profile.
Indirect light: Linear lenses for batwing effect protected by a transparent polycarbonate diffuser.
Fitting accessories ordered separately.

22,4+28W* / 2400+1760lm* / 2200K-5000K / DALI / Wide flood 76° / batwing / 1192mm

LED CRI>80 / >50.000h, L80/B10 / 2-step MacAdam
Power supply included.
IP20 | 230Vac | 50/60Hz

LOR 80%, UGR <19, insulation class I